SPLIT FILM PRINT INSPECTION

Print inspected on October 6th, 2015

Print appears to be in good condition. There were some minor, intermittent emulsion side scratches on the print which appear to be from winding damage or from an improperly set projector loop. These can be seen in images 20151006_123013.jpg, 20151006_123551.jpg, and more. These are very minor and should not affect image. 

Base side only had scratches in the typical edges outside the image area.

The only splices in the film (tail and head) were single spliced. These were replaced with double splices.