FLOW PRINT INSPECTION

Inspected October 6th, 2015.

Films appears to be in good shape. There are several minor base side scratches present in the image area, as seen in 20151006_142048.jpg, 20151006_142218.jpg and other instances. These scratches appear throughout the print, expect for a few sections (mysteriously) in the middle, such as in 20151006_142457.jpg. However, this seems to be an outlaying instance.

The few splices in the film are good. The final tail splice was single splice, which was replaced.

A good amount of the head leader was removed for projection purposes. This will be replaced prior to being returned.